|  |  |  |
| --- | --- | --- |
|  |  |  |
| Động cơ encoder 334 + Diode 1n4007 x5 | 1 | 30k |
| Pc817 | 2 | 6k |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Graphical user interface, text, application, email

Description automatically generated

Graphical user interface, text, application, email

Description automatically generated